­­

PWM max should be set to to achieve max fan speed. IE: map (analogVoltage, 0, 1023, 0, 3400).